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USER MANUAL
Diamond OMNI Digital TV Antenna
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SPECIAL FEATURES
Highlights
360° TV Omni reception

No adjustment needed

Suitable for indoor & outdoor use

Portable for car, camping, marine 
Easy to install and use 

UV protected

PERFORMANCE
Receives Full HD and digital TV signals, local VHF and UHF signals

Built-in wide band amplifier for best performance

360°excellent reception extremely wide frequency range

Connect directly to TV for standard reception
POWERING
To be powered by digital receiver

Or by included AC/DC adaptor

Or 12V adaptor
TECHNICAL SPECIFICATIONS
Frequency:

VHF 174-230MHz UHF 470-694MHz                                     
Impedance (Ω): 75

Polarization: Horizontal

Working Voltage: DC 12V/200mA

Suggest reception range: 0-50 KM from TV transmitters

ACCESSORIES INCLUDED
Adapter, power booster, car charger, F connector, waterproof cap, 3* screws for base, 2*plastic plugs for antennas
WARRANTY & PRODUCT ENQUIRIES
All warranty and product enquiries, contact ONEX – 03 83545500
Manufactured by Team Noble Limited - +86 755 85278182

Check the signal status for your location on this website 
https://myswitch.digitalready.gov.au/
1. Installation Manual
2. Through the cable to the antenna bracketing.
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3. Tighten the screws.
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4. Setting on the caravan.
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Connect:
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